ALT-DVB Beta 105

* Satellite list editor with configurable LNB parameters
  (+ import settings from SatList.def)

* DiseqC functions available for SkyStar1:
  Switch: Committed
  Switch: Uncommitted
  Positioner


* DiseqC functions available for SkyStar2:
- With original driver:
  Switch: Simple   (ToneBurst A/B)
  Switch: Committed 

- With patched driver (by MiBi):
  Switch: Committed
  Switch: Uncommitted
  Positioner

* Option to include PAT stream in .TS recorded file
  (PCR is automaticaly included if <> Video PID)

* EMM updated on channel rescan

* Manually add & delete channel

* Now/Next filters in EPG events

* Basic remote control (WinLirc).For Girder or other RC applications use SendMessage() 
   Message = WM_USER+ 17531 = 18555
   wParam  =
    1 = CH+
    2 = CH-
    3 = VOL+
    4 = VOL-
    5 = MUTE
    6 = FULL SCREEN
    7 = EXIT APP

  .. sorry but no OSD yet :-(
 
  
* Simple ChildLock
  Default password: 179355

* SkyStar1: Teletext through video-out 

----------------------------------------------------

Tested on:
 Windows XP SP1 + DirectX 9b
 SkyStar1 Rev 1.5  + Driver & Firmware 2.16
 SkyStar2 Rev 2.6b + Driver 4.2.8 (original + patched) , 4.2.10 (o+p) , 4.2.11 beta
 Positioner STRONG SRT V50
 Diseq Switch 4x1 (committed)
 