oscam.conf(5)							     File Formats Manual						       oscam.conf(5)



NAME
       oscam.conf - main configuration file for OSCam

SYNOPSIS
       The  main  configuration  file  for  OSCam contains global parameters such as debugging, logging, monitor, protocols and anti-cascading.  sections in
       oscam.conf are nonrecurring. The [global] section is required. All other sections are optional.

DESCRIPTIONS
   The [global] section
       nice = -20..+20
	  system priority, default:99

       pidfile = filename
	  set PID file, default:none

       logfile = [filename][;syslog][;stdout]
	  logging targets, default:/var/log/oscam.log. You can define a maximum of one filename and additionally to log to stdout or syslog  (you  can	also
	  only log to stdout or syslog and omit the filename).
       PP initial_debuglevel = level
	  set initial debug level for OSCam start, default:0
       PP sysloghost = hostname
	  set remote syslog host, default:none

       syslogport = port
	  set TCP/IP port for remote syslog host, default:none

       ecmfmt = format
	  define ECM log format, default:c&p/i/s/l:h

	  possible variables:

	    c = CAID
	    d = PID
	    e = CSP hash
	    g = ID of origin gbox peer
	    h = checksum
	    i = channel ID
	    j = distance of gbox hops
	    l = length
	    o = ONID
	    p = provider ID
	    s = service ID
	    w = CW
	    y = payload

	  use a value as prefix to hide variable with this value, control characters will be escaped by "\"

	   example: ecmfmt = c&0p/i/d/s/l:h.e_w
		    (hide provider ID if 0)

       loghistorylines = lines
	  size of log message history in web interface or monitor, 0 = disabled, default:256

       maxlogsize = kbytes
	  maximum log file size, 0 = unlimited, default:10

       logduplicatelines = 0|1
	  1 = enable logging of duplicate lines in the log, default:0

       disablelog = 0|1
	  1 = disable log file, default:0

       cwlogdir = path
	  directory for CW logging, default:config dir

       emmlogdir = path
	  directory for EMM logging, default:config dir

       usrfile = filename
	  log file for user logging, default:none

	  log file format:

	   date
	   time
	   CWs per second
	   username
	   IP address of client
	   TCP/IP port
	   CWs found
	   CWs from cache
	   CWs not found
	   CWs ignored
	   CWs timed out
	   CWs tunneled
	   login time in unix/POSIX format
	   logout time in unix/POSIX format
	   protocol

       disableuserfile = 0|1
	  1 = avoid logging although userfile is set, default:1 (also set automatically if userfile is empty)

       usrfileflag = 0|1
	  usrfile logging mode:

	    0 = only client logon/logoff will be logged in usrfile (default)
	    1 = each zapping of a client will be logged in usrfile

       disablemail = 0|1
	  1 = disable saving NDS Videoguard mail messages from provider, default:1

       mailfile = file
	  define file saving NDS Videoguard mail messages from provider, default:none

       enableled = 0|1|2
	   0 = LED support disabled (default)
	   1 = LED support enabled for routers
	   2 = LED support enabled for Qbox HD

       waitforcards = 0|1
	  1 = wait for local SCs on startup before opening network ports, default:1

       waitforcards_extra_delay = delay
	  additional delay in milli-seconds after waiting for local SCs on startup before opening network ports, default:500

       preferlocalcards = 0|1
	  SC decoding behavior:

	   0 = local SCs used like a remote reader
	   1 = prefer cache exchange based SCs (default)
	   2 = prefer local SCs

       readerrestartseconds = seconds
	  seconds beetween restarts, 0 = disable reader restart, default:5

       block_same_ip = 0|1
	  1 = reject looping ECMs from clients to readers with the same IP address, default:1

       block_same_name = 0|1
	  1 = reject looping ECMs from clients to readers with the same name, default:1

       clienttimeout = milli-seconds|seconds
	  value (clienttimeout in seconds < 100, else milli-seconds) for client process to wait for key, default:5

       clientmaxidle = seconds
	  value for client process being idle before disconnect, 0 = idle disconnect disabled, default:120

       suppresscmd08 = 0|1
	  0  =	tell  camd 3.5x, 3.57x and 3.78x clients not to request again for rejected CAID, service ID and provider ID combination, 1 = disable, can be
	  overwritten per user in oscam.user, default:0

       fallbacktimeout = milli-seconds
	  time falling back to fallback reader, default:2500

       fallbacktimeout_percaid = milli-seconds
	  time falling back to CAID restricted fallback reader, default:2500

       sleep = minutes
	  time waiting for inactive users, default:none, can be overwritten per user in oscam.user

       serverip = IP address
	  bind service to specified IP address, default:none

       bindwait = seconds
	  value to wait for bind request to complete, default:120

       netprio = 0|1|2|3|4|5|6|7|8|9|10|11|12|13|14|15|16|17|18|19|20
	  value for network priority:
	  IPP value will be applied to SO_PRIORITY (system internal prioritization)
	  DSCP value will be applied to IP_TOS/IPV6_TCLASS (the TOS field in the IP packet header)

	    0 = IPP=0; DSCP=CS0 (default)
	    1 = IPP=1; DSCP=CS1
	    2 = IPP=1; DSCP=AF11
	    3 = IPP=1; DSCP=AF12
	    4 = IPP=1; DSCP=AF13
	    5 = IPP=2; DSCP=CS2
	    6 = IPP=2; DSCP=AF21
	    7 = IPP=2; DSCP=AF22
	    8 = IPP=2; DSCP=AF23
	    9 = IPP=3; DSCP=CS3
	   10 = IPP=3; DSCP=AF31
	   11 = IPP=3; DSCP=AF32
	   12 = IPP=3; DSCP=AF33
	   13 = IPP=4; DSCP=CS4
	   14 = IPP=4; DSCP=AF41
	   15 = IPP=4; DSCP=AF42
	   16 = IPP=4; DSCP=AF43
	   17 = IPP=5; DSCP=CS5
	   18 = IPP=5; DSCP=EF
	   19 = IPP=6; DSCP=CS6
	   20 = IPP=7; DSCP=CS7

       resolvegethostbyname = 0|1
	  set mode for DNS resolving:

	    0 = getadressinfo (default)
	    1 = gethostbyname

       failbancount = count
	  number of incorrect logins after an ip address will be blocked, default:0

       failbantime = minutes
	  time for IP based blocking for clients with an invalid login attempt, 0 = failban is disabled, default:0

       dropdups = 0|1
	  mode for duplicate client connections (requirement: uniq > 0):

	    0 = mark client as duplicate, but don't disconnect them (default)
	    1 = drop duplicate connections instead of marking as duplicate

       unlockparental = 0|1
	  1 = unlock parental mode option to disable Seca and Viaccess pin code request for adult movie, default:0

       double_check = 0|1
	  1 = ECM will be send to two or more readers with the same SC and the CWs will be verified against each other, lb_nbest_readers must be set to 2 or
	  higher, default:0

       double_check_caid = [CAID1|first two digits of CAID1],[CAID2|first two digits of CAID2]...
	  ECM  will  be  send to two or more readers with the same SC and the CWs will be verified against each other for defined CAID or first two bytes of
	  CAID, lb_nbest_readers must be set to 2 or higher, default:none
       getblockemmauprovid = 0|1
	  1 = server overrides EMM blocking defined on client site, default:0

       lb_mode = mode
	  load balancing mode:

	   0 = load balance disabled, ECMs go to all readers (default)
	   1 = fastest reader first, after 5 ECMs the reader with the fastest
	       response time will be selected
	   2 = oldest reader first, reader with the longest no answer
	   3 = lowest usage level, the usage level will be calculated by the
	       sum of 5 ECMS response times, the higher a reader is busy, the
	       higher is usage level

       lb_save = 0|counts
	  save auto load balance statistics:

		0 = saving of auto load balance statistics disabled (default)
	   counts = save auto load balance statistics every counts ECMs
		    (minimum 100)

	  To save CPU power a minimum counts of 100 is recommended.

       lb_nbest_readers = counts
	  set count of best readers for load balancing, default:1

       lb_nfb_readers = counts
	  set count of fallback readers for load balancing, default:1

       lb_nbest_percaid = CAID1:count1[,CAID2:count2]...
	  set count of best readers per CAIDs for load balancing, wildcard CAIDs with two-digit CAIDs possible, default:none

	   example: lb_nbest_percaid = 0100:4,0200:3,03:2,04:1
		    (wildcard CAIDs 03xx and 04xx)

       lb_min_ecmcount = counts
	  minimal ECM count to evaluate load balancing values, default:5

       lb_max_ecmcount = counts
	  maximum ECM count before resetting load balancing values, default:500

       lb_reopen_seconds = seconds
	  time between retrying failed load balanced readers/CAIDs/providers/services, default:900

       lb_reopen_invalid = 0|fB1
	  0 = E_INVALID will be blocked until statistics has been cleaned, default:1

       lb_force_reopen_always = 0|1
	  1 = force reopening immediately all failing readers if no matching reader was found, default:0

       lb_retrylimit = milli-seconds
	  retry next load balanced reader only if response time is higher then lb_retrylimit, default:0

       lb_savepath = filename
	  filenanme for saving load balancing statistics, default:/tmp/.oscam/stat

       lb_stat_cleanup = hour
	  hours after the load balancing statistics will be deleted, default:336

       lb_retrylimits = CAID1:time1[,CAID2:time2]...
	  load balancing retry limit time per CAID, wildcard CAIDs with two-digit CAIDs possible, default:none

	   example: lb_retrylimits = 12:0100,34:0200,5678:0300
		    (wildcard CAIDs 12xx and 34xx)

       lb_noproviderforcaid = CAID1[,CAID2]...
	  ignore provider information for CAIDs to reduce load balancing statistic data, wildcard CAIDs with two-digit CAIDs possible, default:none

	   example: lb_noproviderforcaid = 0100,02,0300,04
		    (wildcard CAIDs 02xx and 04xx)

       lb_max_readers = limit
	  restrict the reader count to limit during load balancing learning:

	       0 = unlimited (default)
	   limit = restrict load balancer readers to limit

       lb_auto_timeout = 0|1
	  1 = enable automatic timeout based on load balancing statistics, default:0

       lb_auto_timeout_p = percent
	  percent added to average time as timeout time, default:30

       lb_auto_timeout_t = milli seconds
	  minimal time added to average time as timeout time, default:300

       lb_auto_betatunnel = 0|1
	  1 = enable automatic Betacrypt tunneling detection for CAIDs 1801, 1833, 1834, and 1835 for load balancing, Betacrypt defintion in oscam.user with
	  betatunnel will be prefered, default:1

       lb_auto_betatunnel_mode = 0|1|2
	  set mode for automatic Betacrypt tunneling:

	   0 = CAID 18XX tunneling to CAID 17X2 only (default)
	   1 = CAID 18XX tunneling to CAID 17X2 and CAID 17X2 tunneling to CAID 18XX (CAID 1833/1801)
	   2 = CAID 18XX tunneling to CAID 17X2 and CAID 17X2 tunneling to CAID 18XX (CAID 1833/1834)
	   3 = CAID 18XX tunneling to CAID 17X2 and CAID 17X2 tunneling to CAID 18XX (CAID 1833/1835)
	   4 = CAID 17X2 tunneling to CAID 18XX (CAID 1833/1801 only)
	   5 = CAID 17X2 tunneling to CAID 18XX (CAID 1833/1834 only)
	   6 = CAID 17X2 tunneling to CAID 18XX (CAID 1833/1835 only)

       lb_auto_betatunnel_prefer_beta = direction
	  set direction for automatic Betacrypt/Nagravision selection:

	     0 = disabled (default)
	     1 = always Betacrypt
	   105 = represents the middle
	   200 = always Nagravision

   The [monitor] section
       port = 0|port
	  UDP port for monitor, 0 = monitor disabled, default:0

       serverip = IP address
	  bind service to specified IP address, default:all

       nocrypt = IP address|IP address range[,IP address|IP address range]...
	  unsecured monitor connection, default:none

	   example: nocrypt = 127.0.0.1,192.168.0.0-192.168.255.255

       aulow = minutes
	  time no EMM occurs so that client is set to low, switch from status "active" to "on", default:30

       monlevel = 0|1|2|3|4
	  monitor level:

	   0 = no access to monitor
	   1 = only server and own procs
	   2 = all procs, but viewing only (default)
	   3 = all procs, reload of oscam.user possible
	   4 = complete access

	  monlevel can be overwritten per user in oscam.user.

       hideclient_to = seconds
	  time to hide clients in the monitor if not sending requests, 0 = disabled, default:25

   The [webif] section
       httpport = [+]port
	  port for web interface, 0 = disabled, praefix + = enable SSL, default:none, required

       httpcert = file
	  file for http SSL certificate, default:oscam.pem

       httpforcesslv3  = 0|1
	  1 = force using SSLv3, default:0

       httpuser = username
	  username for password protection, default:none

       httppwd = password
	  password for password protection, default:none

       httpcss = path
	  path for external CSS file, default:none

       http_prepend_embedded_css = 0|1
	  1 = embedded CSS will be added before external CSS , default:0

       httptpl = path
	  path	for  external  templates and picons, multiple simultaneously templates and picons are possible by creating sub folders (maximum length of 32
	  alphanumeric characters), sub folders naming is corresponding to sub folder in URL, default:none

	   example: httptpl = /this/is/my/path

		    folder with multiple templates:
		      /this/is/my/path/template1
		      /this/is/my/path/template2

		    valid URLs:
		     http://host:port/template1
		     http://host:port/template2

       httpjscript = path
	  path for oscam.js javascript, default:none

       httprefresh = seconds
	  status refresh in seconds, default:none

       httphideidleclients = 0|1
	  1 = enables hiding clients after idle time set in parameter hideclient_to, default:0

       httphidetype = type[type]...
	  characters defining columns to hide in web interface status page (see type column), default:none

	   types:

	   'c': client
	   'h': http
	   'm': monitor
	   'p': proxy
	   'r': reader
	   's': server
	   'x': cache exchange

       httpscript = path
	  path to an executable script which you wish to start from web interface, default:none

       httpallowed = IP address|IP address range[,IP address|IP address range]...
	  http web interface connections allowed, default:127.0.0.1,192.168.0.0-192.168.255.255,10.0.0.0-10.255.255.255,::1

	   example: httpallowed = 127.0.0.1,192.168.0.0-192.168.255.255

       httpdyndns = hostname[,hostname][,hostname]
	  http web interface connections allowed, default:none

	   example: httpdyndns = host.example.com
		    httpdyndns = host1.example.com,host2.example.com

       httpsavefullcfg = 0|1
	  write config:

	   0 = all not empty parameters, all not default parameters, all
	       parameters not containing the same value as the same
	       parameter in global configuration (default)
	   1 = all parameters

       httpoverwritebakfile = 0|1
	  1 = overwrite backup configuration files, default:0

       httpreadonly = 0|1
	  1 = read only modus for web interface, default:0

       httpshowpicons = 0|1
	  1 = show picons in user list, default:0

       httppiconpath = path
	  path to picons, default:none

       httphelplang = en|de|fr|<available wiki languages>
	  set right language for wiki entry point, default:en

       httplocale = environment
	  set the locale environment, default:none

   The [lcd] section
       httposcamlabel = text
	  set individual label in web interface header, default:OSCam

       enablelcd = 0|1
	  1 =enable LCD output, default:0

       lcd_outputpath = path
	  path for LCD output, default:/tmp

       lcd_hideidle = 0|1
	  1 = hide reader in LCD output if reader idle > 20 seconds, default:0

       lcd_writeintervall = seconds
	  LCD refresh interval (minimum 5), default:10

   The [cache] section
       delay = milli-seconds
	  value to delay cached requests, default:0

       max_time = seconds
	  maximum time CWs resist in cache, the time must be 2 seconds highter than the parameter clienttimeout, default:15

       max_hit_time = seconds
	  maximum time for cache exchange hits resist in cache for evaluating wait_time, default:15

       wait_time = [caid][&mask][@provid][$servid][:awtime][:]dwtime[,[caid][&mask][@provid][$servid][:awtime][:]dwtime]...
	  wait time in milli-seconds for cache exchange and Cardservproxy before sending ECMs to reader or proxy, default:none

	   example: wait_time = 0:50:250,0200@00009X:50:150,15:950,0500@000001:150,1602&ffdf:1200

       cacheexenablestats = 0|1
	  1 = enable statistics for cache exchange mode, default:0

	  Please consider memory consumption.

       cacheex_cw_check = [caid][&mask][@provid][$servid]:mode:counter[,[caid][&mask][@provid][$servid]:mode:counter]...

	   mode = specify behaviour for counter:

		  0 = when wait_time expires, serve highest counter's CW
		      got anyway, even if no counter reached (default)
		  1 = never serve CW from cache exchange stored in cache,
		      if it's counter not reaches counter. When wait_time
		      expires, requests will go to normal readers

	   counter = set minimum CW counter to allow CW is used, default:1

       cacheex_mode1_delay = CAID1:time,[BCAID2:time]...
	  delay in milli-seconds for asking cache exchange mode 1 readers, default:none

       csp_port = port
	  UDP port of Cardservproxy for cache exchange, default:none

       csp_serverip = IP
	  bind Cardservproxy for cache exchange to specified IP address, default:none

       csp_ecm_filter = [caid][&mask][@provid][$servid][,[caid][&mask][@provid][$servid]]...
	  Cardservproxy incoming ECM filter setting, default:none

       csp_allow_request = 0|1
	  allow incoming ECM request from Cardservproxy, default:1

       csp_allow_reforward = 0|1
	  1 = reforward other cacheex updates to Cardservproxy peers, option could cause loops, default:0

       cwcycle_check_enable = 0|1
	  1 = enable CW cycle check, default:0

       cwcycle_check_caid = CAID[,CAID]...
	  CAID enabled for CW cycle check, default:none

       cwcycle_maxlist = count
	  maximum CW cycle list entries, default:500, maximum:4000

       cwcycle_keeptime = minutes
	  minimum time a learned cycle time resists in memory, default:15, maximum:15

       cwcycle_onbad = 0|1
	  0 = log bad CW cycle only, 1 = drop bad CW cycle, default:1

       cwcycle_dropold = 0|1
	  1= drop old CW cycle, default:1

       cwcycle_sensitive = 0|2|3|4
	  drop CW mode:

	   0 = disabled
	   2 = 2 (or more) same bytes and drop new CW
	   3 = 3 (or more) same bytes and drop new CW
	   4 = 4 (or more) same bytes and drop new CW (default)

       cwcycle_allowbadfromffb = 0|1
	  1 = allow bad cycles from a fixed fallback reader, default:0

       cwcycle_usecwcfromce = 0|1
	  1 = use CW info from cache exchange, default:0

       wait_until_ctimeout = 0|1
	  answer when cache exchange timeout expires, if no normal readers are available for sending ECMs:

	   0 = immediately send 'not found' to client (default)
	   1 = wait for cache exchange answer until client timeout expires

   The [camd33] section
       port = 0|port
	  TCP port for camd 3.3x clients, 0 = disabled, default:0

       serverip = IP address
	  bind service to specified IP address, default:all

       nocrypt = IP address|IP address range[,IP address|IP address range]...
	  unsecured camd 3.3x client connection, default:none

	   example: nocrypt = 127.0.0.1,192.168.0.0-192.168.255.255

       passive = 0|1
	  1 = force passive camd 3.3x client, default:0

       key = 128 bit key
	  key for camd 3.3x client encryption, default:none

	   example: key = 01020304050607080910111213141516

   The [cs357x] section
       port = 0|port
	  UDP port for camd 3.57x clients, 0 = disabled, default:0

       serverip = IP address
	  bind service to specified IP address, default:all

       suppresscmd08 = 0|1
	  0 = tell camd 3.5x / 3.57x clients not to request again for rejected CAID, service ID and provider ID combination, 1 = disable, can be overwritten
	  per user in oscam.user, default:0

   The [cs378x] section
       port = 0|port[@CAID][:provid][,provid]...[;port@CAID[:provid][,provid]...]...
	  TCP port/CAID/provid definitions for camd 3.78x clients, 0 = disabled, default:0

	   examples: port = 10000@0100:100000;20000@0200:200000,300000,400000
		     port = 30000

       serverip = IP address
	  bind service to specified IP address, default:all

       keepalive = 0|1
	  0 = disable camd 3.78x keepalive modus, default:0

       suppresscmd08 = 0|1
	  0  =	tell  camd 3.78x clients not to request again for rejected CAID, service ID and provider ID combination, 1 = disable, can be overwritten per
	  user in oscam.user, default:0

   The [newcamd] section
       key = DES key
	  default key for newcamd client encryption, default:none

	   example: key = 0102030405060708091011121314

       port = port[{DES key}]@CAID[:provid][,provid]...[;port[{DES key}]@CAID[:provid][,provid]...]...
	  TCP port/DES key/CAID/provid definitions, default:none

	   example: port = 10000@0100:100000;20000{0102030405060708091011121314}@0200:200000,300000

	  Each CAID requires a separate port. If you don't specify a DES key for a port, the default DES key will be used.

       serverip = IP address
	  bind newcamd service to specified IP address, default:all

       allowed = IP address|IP address range[,IP address|IP address range]...
	  newcamd client connections allowed from, default:none

	   example: allowed = 127.0.0.1,192.168.0.0-192.168.255.255,::1

       keepalive = 0|1
	  0 = disable newcamd keepalive modus, default:0

       mgclient = 0|1
	  1 = provide share information of all available CAIDs and provider IDs to mgcamd clients, default:0

   The [radegast] section
       port = 0|port
	  TCP/IP port for radegast clients, 0 = disabled, default:0

       serverip = IP address
	  bind service to specified IP address, default:all

       allowed = IP address|IP address range[,IP address|IP address range]...
	  client connections allowed from, default:none

	   example: allowed = 127.0.0.1,192.168.0.0-192.168.255.255

       user = username
	  user name for radegast client

   The [serial] section
       device = <user>@<device>[:baud][?option1=value1[&option2=value2]...]
		[;<user>@<device>[:baud][?option1=value1[&option2=value2]...]]...

	  parameters:
	   user   = account
	   device = serial device name|hostname|IP,port
	   baud   = serial port speed (for serial devices only)
	   option = timeout = milli-seconds, timeout for connection,
			      default:50
		    delay   = milli-seconds, additional delay between two
			      characters, default:0

	  supported serial devices (autodection):
	   HSIC    (humax sharing interface client)
	   SSSP    (simple serial sharing protocol)
	   bomba   (BOMBA firmware)
	   dsr9500 (DSR 9500)

	   example: user1@/dev/ttyS1:115200?delay=1&timeout=5000
		    user2@192.160.0.1,12345?delay=1&timeout=5000

   The [cccam] section
       port = 0|port[,0|port]...
	  TCP/IP ports for CCcam clients, 0 = disabled, default:0

       version = <main version>.<version>.<sub version>
	  define CCcam version, minimum CCcam version 2.0.11, used with original CCcam only, default:none

	   example: version = 1.2.34

       reshare = level
	  reshare level for CCcam clients (default:10):

	  -1 = no resharing
	   0 = resharing for direct peer only
	   1 = resharing for direct peer and next level
	   x = resharing for direct peer and next x level

       reshare_mode = mode
	  CCcam reshare mode:

	   0 = reader reshares only received SCs for CCcam readers,
	       defined filters/CAIDs/provids on other readers
	   1 = reader reshares received SCs (like=0) and defined services
	   2 = reader reshares only defined reader services as virtual SCs
	   3 = reader reshares only defined user services as virtual SCs
	   4 = reader reshares only received SCs (default)

	  Every server is shared as hop = 0 and with defined reshare values.

	  Service reshare only works if positive services defined: no service - no reshare!

       ignorereshare = 0|1
	  CCcam reshare setting:

	   0 = use reshare setting of server (default)
	   1 = use reshare setting of reader or user

       stealth = 0|1
	  1 = behaviour like the original CCcam: no activate partner detection and extended OSCam-CCcam protocol, prevent other OSCam to detect  the  server
	  as OSCam server, default:0

       minimizecards = mode
	  mode how to provide CCcam servers to CCcam clients:

	   0 = no aggregation, remove duplicates only (default)
	   1 = based on minimum hop: two SCs with different hops are
	       summarized, new SCs get a smaller hop
	   2 = aggregation based on CAIDs: all SCs with the same CAIDs
	       will be merged, provider (maximum 32) will be merged, too

       updateinterval = seconds
	  interval to provide share list update to CCcam clients, values <= 10 are invalid and will be set to 30, default:240

       keepconnected = 0|1
	  set CCcam keepalive modus:

	    0 = disconnect client when maximum idle time is reached
	    1 = keep client connected (default)

       recv_timeout = milli-seconds
	  set network timeout for receiving data, default:2000

       forward_origin_card = 0|1
	  1 = forward ECM request to reader holding this card, load balancer, fallback and caching will be disabled, default:0

       nodeid = ID
	  set CCcam node ID in hex, default:none

	   example: nodeid = 0a0b0c0d0e0f1011

   The [gbox] section
       hostname = hostname| IP address
	  set hostname or IP address for gbox protocol, default:none

       port = port[,port]...
	  UDP port for gbox server, default:0

       my_password = password
	  password for connection to local gbox peer, default:none

       proxy_card = <CAID><provid>[,<CAID><provid>]...
	  proxy reader SCs to be reshared into gbox network, default:none

       ccc_reshare = 0|1
	  1 = enable CCCam reshare, default:0

       my_vers = version
	  set gbox version in hexadecimal low byte, default:2A

       my_cpu_api = byte
	  set gbox CPU and API byte in hexadecimal, default:40

       gbox_reconnect = time
	  send message to peers in seconds, default:180, min:60, max:300

       log_hello = 0|1
	  1 = log hello messages ,default:1

       dis_attack_txt = 0|1
	  1 = disable creation of file attack.txt ,default:0

       gsms_disable = 0|1
	  1 = disable gbox short message service (GSMS),default:1

	  sending  a  messeage:  /tmp/gsms.txt:  <box  ID>  <1=mormal  message|2=OSD/TV  message>  <message  6	to 127 characters>, status will be stored in
	  '/tmp/gsms.ack' respective 'gsms.nack', receiving a message: The message will be stored in /tmp/gsms.log

       tmp_dir = path
	  temporary directory for gbox, default:/tmp/.oscam

       accept_remm_peer = peer-id1[,peer-id2]...
     accept REMM requests from gbox peer(s), default:none

   The [scam] section
       port = port
	  UDP port for scam server, default:0

   The [dvbapi] section
       enabled = 0|1
	  1 = DVB API enabled, default:0

	  Create file /tmp/.pauseoscam to pause DVB API, e.g. if STB goes into standby and OSCam remains as SC server only.

       listen_port = 0|port
	  TCP/IP port for SAT IP clients, filtering has to be done on client site, 0 = disabled, default:0

       user = username
	  user name for DVB API client, default:anonymous

       ignore = <CAID>[,<CAID>]... (detached by oscam.dvbapi, obsolete)
	  CAIDs to be ignored, default:none

       services = <service ID>[,<service ID>]... (detached by oscam.dvbapi, obsolete)
	  services to be prioritized, default:none

       priority = <CAID>:<provider ID>[,CAID:<provider ID>]... (detached by oscam.dvbapi, obsolete)
	  CAIDs and provider IDs to be prioritized, default:CAIDs and provider IDs of local SCs will be prioritized

       au = 0|1
	  AU mode:

	   0 = disable AU (default)
	   1 = enable AU

       pmt_mode = 0|1|2|3|4|5
	  PMT mode:

	   0 = use camd.socket and PMT file, default
	   1 = disable reading PMT file
	   2 = disable camd.socket
	   3 = read PMT file on startup only
	   4 = do not use signal handler for monitoring /tmp
	   5 = do not use signal handler for monitoring /tmp,
	       disable camd.socket

	   ecminfo_file = 0|1
	  ecm.info types:

	   0 = Disable ecm.info file
	   1 = Enable ecm.info file (default)

       ecminfo_type = 0|1|2|3|4|5
	  ecm.info types:

	   0 = OSCam syntax (default)
	   1 = OSCam syntax with ECM time in ms instead of seconds
	   2 = WiCardd
	   3 = mgcamd
	   4 = CCcam
	   5 = camd3

       request_mode = 0|1
	  CAID request mode:

	   0 = try all possible CAIDs one by one (default)
	   1 = try all CAIDs simultaneously

       boxtype = dbox2|dreambox|dm7000|duckbox|ufs910|ipbox|ipbox-pmt|qboxhd|coolstream|neumo|samygo|pc
	  set boxtype, auto detection of DVB API will be aspired, default:dreambox

	  ipbox with camd.socket support, currently only with PGI image version 0.6 or above, verified on HD models only

	  ipbox-pmt can be used on any DGS based images (with or without camd.socket support), verified on HD models only

	  pc is for generic pc support (currently supported on VDR with vdr-plugin-dvbapi)

       read_sdt = 0|1|2
	  mode of provider, channel name and service type auto detection via SDT:

	   0 = disabled (default)
	   1 = enabled for non FTA channels only
	   2 = enabled for all channels

       write_sdt_prov = 0|1
	  mode writing provider name into oscam.srvid2 file:

	   0 = disabled (default)
	   1 = enabled

       demuxer_fix = 0|1
	  try fixing audio/video sync errors:

	   0 = disabled (default)
	   1 = enabled

       cw_delay = milli-seconds
	  delay of CW writing, default:none

       delayer = milli-seconds
	  minimum time to write CW, default:0

       reopenonzap =  0|1
	  1 = reopen demux devices on each channel switching, default:0

   The [anticasc] section
       enabled = 0|1
	  1 = enable anti-cascading, default:0

       numusers = quantity
	  anti-cascading: user per account, 0 = anti-cascading disabled, default:0

       sampletime = minutes
	  duration of sample, default:2

       samples = quantity
	  quantity of samples over limit, default:10

       penalty = 0|1|2|3
	  level of penalty:

	   0 = only logging (default)
	   1 = send fake CWs
	   2 = temporary user ban
	   3 = send delayed CWs

	  penalty can be overwritten per user in oscam.user.

       aclogfile = filename
	  file for anti-cascading logging, default:none

       fakedelay = milli-seconds
	  fake delay time, default:1000, minimum value is 100, maximum value is 3000

       denysamples = quantity
	  how many samples should be penalized, default:8

       acosc_enabled = 0|1
	  1 = enable anti-cascading over SID count, default:0

       acosc_max_ecms_per_minute = count
	  maximum ecms per minute, 0 = unlimited, default:0

       acosc_max_active_sids = count
	  maximum active SIDs with anti-cascading over SID, 0 = unlimited, default:0

	  Can be overwritten per user in oscam.user.

       acosc_zap_limit = count
	  zap limit for anti-cascading over SID, 0 = unlimited, default:0

	  Can be overwritten per user in oscam.user.

       acosc_penalty = 0|1|2|3|4
	  level of penalty with anti-cascading over SID count:

	   0 = only logging (default)
	   1 = send fake CWs
	   2 = temporary user ban
	   3 = send delayed CWs
	   4 = temporary hidecards to the client

	  Can be overwritten per user in oscam.user.

       acosc_penalty_duration = seconds
	  penalty duration for anti-cascading over SID count, default:0

	  Can be overwritten per user in oscam.user.

       acosc_delay = milli-seconds
	  delay for anti-cascading over SID count, default:0

	  Can be overwritten per user in oscam.user.

LOGGING
       ·  reader stages

	   1 = cacheex (=1) reader (C)
	   2 = local SCs (L)
	   3 = other reader / proxies (P)
	   4 = fallback reader (F)

       ·  logging format

	   stage/used/chosen/possible

MONITOR
       monitor commands:

       ·  login <user> <password>

	  login (for unencrypted connections only)


       ·  getuser <user> <parameter>=<value>

	  get parameter for user


       ·  setuser <user> <parameter>=<value>

	  set parameter for user


       ·  setserver <parameter>=<value>

	  set parameter for server


       ·  exit

	  exit monitor


       ·  log <on|onwohist|off>

	  enable|enable without hitory|disable logging for 2 minutes


       ·  status

	  list of current processes and clients


       ·  shutdown

	  shutdown OSCam


       ·  restart

	  restart OSCam


       ·  keepalive

	  send keepalive


       ·  reload

	  reinit user db, clients and anti-cascading, for newcamd connections: after reloading the provid, please restart newcamd client


       ·  details <PID>

	  details about selected PID


       ·  reread

	  read again


       ·  debug <level>

	  set debug level (monlevel > 3 required)

	  debug level mask:
	       0 = no debugging (default)
	       1 = detailed error messages
	       2 = ATR parsing info, ECM dumps, CW dumps
	       4 = traffic from/to the reader
	       8 = traffic from/to the clients
	      16 = traffic to the reader-device on IFD layer
	      32 = traffic to the reader-device on I/O layer
	      64 = EMM logging
	     128 = DVB API logging
	     256 = load balacing logging
	     512 = cache exchange logging
	    1024 = client ECM logging
	   65535 = debug all

       ·  version

	  show OSCam version


       ·  commands

	  show all valid monitor commands

WEB INTERFACE
       ·  template system

	  The web interface allows you to create your own template. For developing your own template request the orignal template with the  non-linked	page
	  savetemplates.html. Store your own template in the directory specified by httptpl.

CACHING
       types of ECM caching:

       ·  cache1

	  ECM and CW in cache already.

       ·  cache2

	  ECM and checksum in cache already.

SEE ALSO
       list_smargo(1), oscam(1), oscam.ac(5), oscam.cacheex(5), oscam.cert(5), oscam.dvbapi(5), oscam.fakecws(5), oscam.guess(5), oscam.ird(5),
       oscam.provid(5), oscam.ratelimit(5), oscam.server(5), oscam.services(5), oscam.srvid(5), oscam.srvid2(5), oscam.tiers(5), oscam.user(5),
       oscam.whitelist(5)



																	       oscam.conf(5)
