Reader specific settings for Nagra Merlin
Init card in CAK7 mode:
Force CW swap:
Force Even SA:
Force EMMs 0x82:
mod1:##MOD1##
mod2:##MOD2##
key3588:##KEY3588##
key3460:##KEY3460##
key3310:##KEY3310##
data50:##DATA50##
mod50:##MOD50##
idird:
CMD0E ProvID: use only if CMD0E needs ProvID other than sysid
Nuid:
Force Pairing (00 - global):
Force OTP CSC (optional):
Force OTA CSC (optional):
CaID BoxEMM:
OTA (Over-The-Air) CWPK:
Header mode:
CWPK0:
CWPK1:
CWPK2:
CWPK3:
CWPK4:
CWPK5:
CWPK6:
CWPK7:
CWPK8:
CWPK9:
CWPK10:
CWPK11:
CWPK12:
CWPK13:
CWPK14:
CWPK15:
CWPK16: