oscam.ratelimit(5)				       File Formats Manual				       oscam.ratelimit(5)



NAME
       oscam.ratelimit - ECMs ratelimit for OSCam

SYNOPSIS
       limit rate of ECMs allowed for an interval

DESCRIPTIONS
       CAID:provider ID:service ID:ChID:ratelimitecm:ratelimitseconds:srvidholdseconds

	  ratelimitecm
	     number of different SIDs in ECMs allowed for an interval

	  ratelimitseconds
	     interval in seconds for ratelimit

	  srvidholdseconds
	     extra time in seconds this service ID is kept in a slot before another service ID can take its place

EXAMPLES
	0100:00002A:3A3A:4A00:0002:0010:0004

SEE ALSO
       list_smargo(1), oscam(1), oscam.ac(5), oscam.cacheex(5), oscam.cert(5), oscam.conf(5), oscam.dvbapi(5), oscam.fakecws(5),
       oscam.guess(5), oscam.ird(5), oscam.provid(5), oscam.server(5), oscam.services(5), oscam.srvid(5), oscam.srvid2(5),
       oscam.tiers(5), oscam.user(5), oscam.whitelist(5)



													       oscam.ratelimit(5)
